Calculation of non-dimensional C

is the concentration in ppm.

is the wind velocity at , .

is taken as 0.216m, which is taken as the midpoint between the two larger buildings NW1 and SE which are 0.212m and 0.220m respectively.

is the tunnel wind velocity.

is the flow rate of the tracer gas hydrocarbon.